# **REQUEST FOR QUOTATION (RFQ)**

|  |  |
| --- | --- |
| RFQ Reference: **RFQ/PAK/December/2022/069** | Date: 06 December 2022 |

# **SECTION 1: REQUEST FOR QUOTATION (RFQ) for the Repair/Rehabilitation works in 6-PHED schemes in Quetta Balochistan under QIPS**

International Organisation for Migration (IOM) kindly requests your quotation for the provision of goods, as detailed in Annex 1 of this RFQ.

This Request for Quotation comprises the following documents:

Section 1: This request letter

Section 2: RFQ Instructions and Data

Annex 1: Schedule of Requirements

Annex 2: Quotation Submission Form

Annex 3: Technical and Financial Offer

When preparing your quotation, please be guided by the RFQ Instructions and Data. Please note that quotations must be submitted using Annex 2: Quotation Submission Form and Annex 3 Technical and Financial Offer, by the method and by the date and time indicated. It is your responsibility to ensure that your quotation is submitted on or before the deadline. Quotations received after the submission deadline, for whatever reason, will not be considered for evaluation.

Thank you and we look forward to receiving your quotations.

Approved by:

Signature:

Name: Abeer Alami

Title: Procurement and Logistics Officer

Date: 02/12/2022

## **SECTION 2: RFQ INSTRUCTIONS AND DATA**

|  |  |
| --- | --- |
| **Deadline for the Submission of Quotation** | **14 December 2022**If any doubt exists as to the time zone in which the quotation should be submitted, refer to <http://www.timeanddate.com/worldclock/>. |
| **Method of Submission** | Quotations must be submitted as follows: [ ]  E-tendering[x]  Email[ ]  Courier / Hand delivery[ ]  Other Click or tap here to enter text.Bid submission address: **pakbids@iom.int*** File Format: PDF
* File names must be maximum 60 characters long and must not contain any letter or special character other than from Latin alphabet/keyboard.
* All files must be free of viruses and not corrupted*.*
* Max. File Size per transmission: 4MB
* Mandatory subject of email: **RFQ/PAK/December/2022/069 Repair/Rehabilitation works in 6-PHED schemes in Quetta Balochistan under QIPS**
* Multiple emails must be clearly identified by indicating in the subject line “email no. X of Y”, and the final “email no. Y of Y.
* It is recommended that the entire Quotation be consolidated into as few attachments as possible.
* The proposer should receive an email acknowledging email receipt.
 |
| **Cost of preparation of quotation** | IOM shall not be responsible for any costs associated with a Supplier’s preparation and submission of a quotation, regardless of the outcome or the manner of conducting the selection process. |
| **Supplier Code of Conduct** | All prospective suppliers must read the UN Supplier Code of Conduct and acknowledge that it provides the minimum standards expected of suppliers to the UN. The Code of Conduct, which includes principles on labour, human rights, environment and ethical conduct may be found at: [Supplier Code of Conduct (ungm.org)](https://www.ungm.org/Public/CodeOfConduct).  |
| **Conflict of Interest** | **UN encourages every prospective Supplier to** avoid and prevent conflicts of interest, by disclosing to UN if you, or any of your affiliates or personnel, were involved in the preparation of the requirements, design, specifications, cost estimates, and other information used in this RFQ. |
| **General Conditions of Contract** | Any Purchase Order or contract that will be issued as a result of this RFQ shall be subject to the IOM General Conditions of Contract for provision of goods/services/transportation/medical services available at https://www.iom.int/do-business-us-procurement.  |
| **Eligibility** | Bidders shall have the legal capacity to enter into a binding contract with IOM and to deliver in the country, or through an authorized representative. |
| **Currency of Quotation** | Quotations shall be quoted in **PKR**  |
| **Duties and taxes** | The International Organization for Migration is exempt from all direct taxes, except charges for public utility services, and is exempt from customs restrictions, duties, and charges of a similar nature in respect of articles imported or exported for its official use. All quotations shall be submitted net of any direct taxes and any other taxes and duties, unless otherwise specified below: All prices shall:[x]  be inclusive of VAT and other applicable indirect taxes[ ]  be exclusive of VAT and other applicable indirect taxes |
| **Language of quotation and documentation including catalogues, instructions and operating manuals** | English |
| **Documents to be submitted** | Bidders shall include the following documents in their quotation:[x]  Annex 2: Quotation Submission Form duly completed and signed[x]  Annex 3: Technical and Financial Offer duly completed and signed and in accordance with the Schedule of Requirements in Annex 1[ ]  Other Click or tap here to enter text.  |
| **Quotation validity period** | Quotations shall remain valid for **90** days from the deadline for the Submission of Quotation. |
| **Price variation** | No price variation due to escalation, inflation, fluctuation in exchange rates, or any other market factors shall be accepted at any time during the validity of the quotation after the quotation has been received.  |
| **Partial Quotes** | [x]  Not permitted[ ]  Permitted  |
| **Payment Terms** | [x]  100% within 30 days after receipt of goods, works and/or services and submission of payment documentation.[ ]  Other Click or tap here to enter text.  |
| **Contact Person for correspondence, notifications and clarifications** | Focal Person: Irfan ZafarE-mail address: izafar@iom.intAttention: Quotations shall not be submitted to this address but to the address for quotation submission above. |
| **Clarifications** | Requests for clarification from bidders will not be accepted any later than 01 day before the submission deadline. Responses to request for clarification will be communicated by email by 08 December 2022 |
| **Evaluation method** | [x] The contract will be awarded to the lowest price substantially compliant offer[ ]  Other Click or tap here to enter text. |
| **Evaluation criteria** | [x] Full compliance with all requirements as specified in Annex 1 [x] Full acceptance of the General Conditions of Contract[x] Comprehensiveness of after-sales services[ ] Earliest Delivery /shortest lead time [ ] Others *(for ex, environmental criteria/considerations, etc)*   |
| **Right not to accept any quotation** | IOM is not bound to accept any quotation, nor award a contract or Purchase Order |
| **Right to vary requirement at time of award** | At the time of award of Contract or Purchase Order, IOM reserves the right to vary (increase or decrease) the quantity of services and/or goods, by up to a maximum 25% of the total offer, without any change in the unit price or other terms and conditions. |
| **Type of Contract to be awarded** | Purchase Order  |
| **Expected date for contract award.** | 22 December 2022 |
| **Policies and procedures** | This RFQ is conducted in accordance with Policies and Procedures of IOM  |
| **UNGM registration** | IOM is encouraging all suppliers to register at the United Nations Global Marketplace (UNGM) website at [www.ungm.org](http://www.ungm.org). The Bidder may still submit a quotation even if not registered with the UNGM, however, if the Bidder is selected for Contract award of USD 100,000 and above, the Bidder is recommended to register on the UNGM prior to contract signature. For vendors who do not have the technical means to register in UNGM, the UNGM has implemented an assisted vendor registration functionality that allows IOM procurement personnel to add local vendors to the UNGM.  |

## **ANNEX 1: SCHEDULE OF REQUIREMENTS**

**Technical Specifications for Repair/Rehabilitation works in 6-PHED schemes in Quetta Balochistan under QIPS**

1. **Water Supply Scheme, Killi Jahangeer Abad – Kuchlak**

|  |  |
| --- | --- |
| **A.** | **Supply and Installation of Pumping Machinery at Jahangeerabad Kuchlak WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pump set SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 3" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and acessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class-B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12'X14' Jahangeerabad Kuchlak WSS** |  |
|  |
| **S.No** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| 1 | 4-47-1 | Removing cement or lime plaster from walls (where no scaffolding is required) | Sft | 2240 |  |
| 2 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good damaged surface | Per Point | 4 |  |
| 3 | 30-3-d | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 4 | 30-17 | Supply and install 5 Amp, 250 Volt moulded, one-way, single pole, flush mounting piano type light control switch alongwith fan dimmers on appropriate size plastic box to be fixed recessed in wall alongwith switch box and plate suitable for upto 3 switches on a common board. | Per Point | 3 |  |
| 5 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 6 | 15-4-ii | 3/4 inch (19mm) thick cement plaster using Coarse Sand on walls andcolumns in basement, plinth and ground floor including making edges,corners and curing. 1:3 | Sft | 2240 |  |
| 7 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 216 |  |
| 8 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 9 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ atleast 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 10 | 17-61-b | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 505 |  |
| 11 | NSI | Visibility Board & Painting | Job | 1 |  |

1. **Water Supply Scheme (WSS) of Killi Sanzar Khel, Kuchlak.**

|  |  |
| --- | --- |
| **A.** | **Supply and Installation of Pumping Machinery at SanzarKhel Kuchlak WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pumpset SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 3" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and acessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying, and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12'X14' SanzarKhel Kuchlak WSS** |  |
|  |
| **S#** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| 1 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good, damaged surface | Per Point | 4 |  |
| 2 | 30-3-d | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch-to-switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, New age r approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 3 | 30-17 | Supply and install 5 Amp, 250 Volt molded, one-way, single pole, flush mounting piano type light control switch along with fan dimmers on appropriate size plastic box to be fixed recessed in wall along with switch box and plate suitable for up to 3 switches on a common board. | Per Point | 3 |  |
| 4 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 5 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ at least 1.25Litre per 10 Sq.m) | Sft | 216 |  |
| 6 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 7 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ at least 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 8 | 17-61-b | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 505 |  |
| 9 | NSI | Visibility Board & Painting | Job |   |  |
|  |  |  |  |  |  |

1. **Water Supply Scheme, Killi Kechi Baig – Quetta**

|  |  |
| --- | --- |
| **A.** | **Supply and Installation of Pumping Machinery at Kechi Baig WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pump set SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 2.5" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and accessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc.: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class-B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12X14 - Kechi Baig WSS** |  |
|  |
| **S#** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| 1 | 4-47-1 | Removing cement or lime plaster from walls (where no scaffolding is required) | Sft | 1000 |  |
| 2 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good damaged surface | Per Point | 4 |  |
| 3 | 30-3-d) | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 4 | 30-17 | Supply and install 5 Amp, 250 Volt moulded, one-way, single pole, flush mounting piano type light control switch alongwith fan dimmers on appropriate size plastic box to be fixed recessed in wall alongwith switch box and plate suitable for upto 3 switches on a common board. | Per Point | 3 |  |
| 5 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 6 | 15-4-ii | 3/4 inch (19mm) thick cement plaster using Coarse Sand on walls andcolumns in basement, plinth and ground floor including making edges,corners and curing. 1:3 | Sft | 1000 |  |
| 7 | 5-5-b | Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 1- 1/2" (38mm) & down gauge in foundation including levelling, compacting and curing. | Cft | 105 |  |
| 8 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 88 |  |
| 9 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 10 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ atleast 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 11 | 17-61-b | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 505 |  |
| 12 | NSI | Visibility Board & Painting | Job |   |  |
|  |

1. **Water Supply Scheme, Killi Kot Waal – Quetta**

|  |  |
| --- | --- |
| **A.** | **Supply and Installation of Pumping Machinery at Kotwaal WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pump set SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 3" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and acessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class-B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12'X14' Kotwaal WSS** |  |
|  |
| **S#** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| **(i) Pump House** |  |
| 1 | 4-19-a | Removal/Dismantling of damaged plain cement concrete 1 : 2 : 4 & richer mixes  | Cft | 42 |  |
| 2 | 4-59-1 | Removing cement or lime plaster of any thickness from ceiling and disposing of the rubbish in any floor | Sft | 280 |  |
| 3 | 4-47-1 | Removing cement or lime plaster from walls (where no scaffolding is required) | Sft | 1017.75 |  |
| 4 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good damaged surface | Per Point | 4 |  |
| 5 | 30-3-d | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 6 | (S.I.No. 30-17) | Supply and install 5 Amp, 250 Volt moulded, one-way, single pole, flush mounting piano type light control switch alongwith fan dimmers on appropriate size plastic box to be fixed recessed in wall alongwith switch box and plate suitable for upto 3 switches on a common board. | Per Point | 3 |  |
| 7 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 8 | 15-4-ii | 3/4 inch (19mm) thick cement plaster using Coarse Sand on walls andcolumns in basement, plinth and ground floor including making edges,corners and curing. 1:3 | Sft | 1276 |  |
| 9 | 5-5-b  | Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 1- 1/2" (38mm) & down gauge in foundation including levelling, compacting and curing. | Cft | 105 |  |
| 10 | 14-2-iii | Providing and laying 1:2:4 cement concrete floor using using crushed aggrgate 3/4" (19mm) and down gauge in ground floor laid in panels including formwork, consolidation, finishing and curing. | Cft | 42 |  |
| 11 | 28-49-b | Providing and fixing steel grated single leaf door with 1/16" (1.6mm) thick M.S. sheeting and locking arrangement, angle iron 2"x2"x3/8" frame, middle strip, 1/4" thick gusset plate 3"x3" at each edge and 3/4" M.S square or round bars at 4" c/c including two coats of red oxide paint. | Sft | 28 |  |
| 12 | 28-58-b-i | Providing & fixing steel windows with openable glazed panels using beam section for frame 1.5"x1"x5/8"x1/8" z-section for leave 3/4"x1"x3/4"x1/8" T-section sashes 1"x1"x1/8 " glass panes, wooden screws for glazing embedded over a thin layer of putty duty screwed with leave with fittings of approved make including cost of painting, hold fast, fabrication, cutting holes as per approved design. | Sft | 24 |  |
| 13 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 104 |  |
| 14 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 15 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ atleast 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 16 | 17-61-C | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 640 |  |
| **(ii) 'Boundary Wall** |  |
| 1 | 3-21 A | Excavation in foundation of buildings and bridges including layout, dressing, refilling around structures with excavated earth, watering & ramming lead upto 100 ft. (30m) & lift upto 5 ft. (1.5m). Ordinary Soil | Cft | 121 |  |
| 2 | 5-8 E | Providing and laying cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm) & down gauge in foundation including leveling, compacting and curing. 1:4:8 | Cft | 15.125 |  |
| 3 | 5-8 C | Providing and laying cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm) & down gauge in foundation including leveling, compacting and curing. | Cft | 45.375 |  |
| 4 | 11-3 B | Providing and laying first class solid burnt brick masonry (Brick Strength:1800psi-2000psi) including scaffolding, raking out joints and curing in foundation and substructure/Basement i/c cost of testing. 1:4 | Cft | 31.3 |  |
| 5 | 11-3 b | Providing and laying first class solid burnt brick masonry (Brick Strength:1800psi-2000psi) including scaffolding, raking out joints and curing in foundation and substructure/Basement i/c cost of testing. 1:4 | Cft | 35.94375 |  |
| 6 |  5-49 a | Providing and laying 1:2:4 cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm.) and down gauge in plinth band, door band and roof band of required shape or section including formwork and its removal, compacting and curing in basement and ground floor but excluding the cost of reinforcement. | Cft | 17.5 |  |
| 7 | 11-12 b | Providing and laying first class solid burnt brick masonry (Brick Strength:1800psi-2000psi) including scaffolding, raking out joints and curing in ground floor superstructure and i/c cost of testing. 1:4 | Cft | 112.3875 |  |
| 8 | 11-12 b | Providing and laying first class solid burnt brick masonry (Brick Strength:1800psi-2000psi) including scaffolding, raking out joints and curing in ground floor superstructure and i/c cost of testing. 1:4 | Cft | 56 |  |
| 9 | 5-15 C | Providing and laying in situ cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm) and down gauge in pillars and columns of any shape in super structure including compacting, curing, cost of form-work & its removal in basement and ground floor. | Cft | 93.76875 |  |
| 10 | 11-35-1 | Providing, fabricating and laying muild steel reinforcement for all kinds of R.C.C. work in foundation, plinth and ground floor including the cost of straightening, removal of rust, cutting, bending, binding, wastage and providing such overlaps as are not shown on the drawings. The cost of binding wire and precast 1:2:4 cement concrete spacer blocks or M.S chairs for binding and holding the reinforcement in position in inclusive upto 5m (14.6 ft) height but for deformed bars grade 40, having yield strength equal to 40,000 psi. | Ton | 0.063244 |  |
| 11 | 5-16 A | Providing and laying 1:2:4 cement concrete using approved coarse sand and crushed aggregate 3/4" (19mm) and down gauge in beams, lintels and cantilevers of required shape or section including formwork and its removal compacting and curing in basement and ground floor | Cft | 6.75 |  |
| 12 | 15-36 C | Pointing on brick work with cement sand mortar in plinth and ground floor including raking out joints and curing. Tuck or weather struck pointing in cement sand mortar. 1:3 | Sft | 162 |  |
| 13 | 15-4 | 3/4 inch (19mm) thick cement plaster using Coarse Sand on walls and columns in basement, plinth and ground floor including making edges, corners and curing. 1:4 | Sft | 448 |  |
| 14 | 28-49-b | Providing and fixing steel grated single leaf door with 1/16" (1.6mm) thick M.S. sheeting and locking arrangement, angle iron 2"x2"x3/8" frame, middle strip, 1/4" thick gusset plate 3"x3" at each edge and 3/4" M.S square or round bars at 4" c/c including two coats of red oxide paint. | Sft | 28 |  |
| 15 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 56 |  |
| 16 | 17-61-C | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 336 |  |
| 17 | NSI | Visibility Board & Painting | Job | 1 |  |

1. **Water Supply Scheme, Killi Kharotabad – Quetta**

|  |  |
| --- | --- |
| **A.** | **Supply and Installation of Pumping Machinery at Kharotabad WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pumpset SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 3" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and acessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class-B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12'X14' Kharotabad WSS** |  |
|  |
| **S#** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| 1 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good damaged surface | Per Point | 4 |  |
| 2 | 30-3-d | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 3 | 30-17 | Supply and install 5 Amp, 250 Volt moulded, one-way, single pole, flush mounting piano type light control switch alongwith fan dimmers on appropriate size plastic box to be fixed recessed in wall alongwith switch box and plate suitable for upto 3 switches on a common board. | Per Point | 3 |  |
| 4 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 5 | 5-5-b | Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 1- 1/2" (38mm) & down gauge in foundation including levelling, compacting and curing. | Cft | 90 |  |
| 6 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 232 |  |
| 7 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 8 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ atleast 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 9 | 17-61-b | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 425 |  |
| 10 | NSI | Visibility Board & Painting | Job | 1 |  |

1. **Water Supply Scheme, Killi Sheikh Maanda Ziarat – Quetta**

|  |  |
| --- | --- |
|  **A.** | **Supply and Installation of Pumping Machinery at Sheikh Maanda Ziarat WSS** |
|  |
| **S#** | **Ref: CSR-2018**  | **Description** | **Unit** | **Quantity** |  |
| 1 | NSI | Providing and fixing at Site of 40-HP Submersible Pumpset SS3 04 (Motor 40-HP, Pump 30BP6300) of FELSOM / IRCEM, KSB, Alarko or approved equivalent (similar specifications), complete in all respects. | Nos | 1 |  |
| 2 | 27-60-a-viii | Supply and Install G.I pipe 2.5" IIL or equivalent make registered with PSQCA 27.3.1.1 including the cost of specials and cost of bitumen for 2 coats and specials for Column Pipes. | Rft | 850 |  |
| 3 | 31-3-o | Supply, install, connect, test and commission of CABLES and acessories. Cable - stranded and flexible insulated copper wires and cables must be used for all outdoor and indoor installations. Voltage drop must not exceed 1%. The outer insulation: sunlight (UV)-resistant and weather. | Rft | 950 |  |
| 4 | NSI | Providing, Supplying and fixing of panel board including starter main switch #-No cutouts i.e; complete wiring etc: complete in all respect.  | Nos | 1 |  |
| 5 | 27-29-a | Providing and fixing C.I. sluice valve of BSS quality and weight, class-B, for C.I. pipe line and A.C. pipe line including cost of jointing material. | Nos | 3 |  |
| **B.** | **Rehabilitation of Pump House Size 12'X14' Sheikh Maanda Ziarat WSS** |  |
|  |
| **S#** | **Ref: CSR-2018**  | **Description**  | **Unit** | **Quantity** |  |
| 1 | 4-47-1 | Removing cement or lime plaster from walls (where no scaffolding is required) | Sft | 3500 |  |
| 2 | 4-52-1 | Dismantling light and fan point including casing and capping strip open type and making good, damaged surface | Per Point | 4 |  |
| 3 | 30-3-d | Concealed/open wiring from point to switch with length upto 30 ft. (10m) including any switch to switch wiring with 3x1.5 Sq.mm PVC insulated single core copper conductor Pakistan Cables, Pioneer, Newage or approved equivalent cables, d) Open pipe wiring with M.S. conduit and accessories such as bends, elbows, junction boxes etc. | Per Point | 4 |  |
| 4 | 30-17 | Supply and install 5 Amp, 250 Volt moulded, one-way, single pole, flush mounting piano type light control switch alongwith fan dimmers on appropriate size plastic box to be fixed recessed in wall alongwith switch box and plate suitable for upto 3 switches on a common board. | Per Point | 3 |  |
| 5 | 30-19 | Supply and install combined 2/3 pin 5 Amps, 250 Volt switch socket unit including plastic box to be fixed recessed in wall.  | Per Point | 1 |  |
| 6 | 15-4-ii | 3/4 inch (19mm) thick cement plaster using Coarse Sand on walls andcolumns in basement, plinth and ground floor including making edges,corners and curing. 1:3 | Sft | 3500 |  |
| 7 | 5-5-b  | Providing and laying plain machine mixed cement concrete using coarse sand and crushed aggregate having maximum size upto 1- 1/2" (38mm) & down gauge in foundation including levelling, compacting and curing. | Cft | 105 |  |
| 8 | 17-7 | Painting with ICI/Berger or equivalent super gloss synthetic enamel paint in two or more coats as per manufacturer's instructions on steel and iron work over and including the cost of priming coat, surface preparation, removing rust, scales and dust with wire brush in ground floor or basement. (@ atleast 1.25Litre per 10 Sq.m) | Sft | 88 |  |
| 9 | 17-58 | Painting with Premier Quality Distemper on old surface of walls and ceiling including dusting and cleaning in basement and ground floor. | Sft | 168 |  |
| 10 | 17-8-1 | Painting with ICI/Berger or equivalent plastic emulsion paint of approved shade in two or more coats as per manufacturer's instructions on plastered rendered and/or concrete surface over and including the cost of priming coat, surface preparation, dusting, rubbing down smooth, filling cracks, holes removing blisters and other blisters and other imperfections in ground floor or basement. (@ atleast 1.65 Litre per 10 Sq.m) | Sft | 468 |  |
| 11 | 17-61-b | Applying weather resistant paint coating such as ICI/ Berger or equivalent paint of approved shade on old surface of walls and ceiling including dusting, sand papering and cleaning, scaffolding and removal of debris. | Sft | 505 |  |
| 12 | NSI | Visibility Board & Painting | Job | 1 |  |

**Delivery Requirements**

|  |
| --- |
| **Delivery Requirements** |
| **Delivery date and time** | Delivery period shall be till the mid of the month of January 2023 |
| **Delivery Terms (INCOTERMS 2020)** | Delivery at Place (DAP) |
| **Customs clearance****(must be linked to INCOTERM** | [ ]  Not applicableShall be done by:[ ]  Name of organisation[x]  Supplier/bidder[ ]  Freight Forwarder |
| **Exact Address(es) of Delivery Location(s)** | The goods should be delivered at the following delivery site/s:WSS (Killi Jahangeer Abad, Kuchlak)WSS (Killi Sanzar Khel, Kuchlak)WSS (Killi Kechi Baig, Saryab Road, Quetta)WSS (Killi Kotwall Abad, Nawa Killi, Quetta)WSS (Killi Kharotabad , Sammungli Road, Quetta)WSS (Killi Sheikh Maanda Ziarat, Airport road, Quetta) |
| **Packing Requirements** | Not required |
| **Training on Operations and Maintenance** | Not required |
| **Warranty Period** | 1 year |
| **After-sales service and local service support requirements** | Click or tap here to enter text. |
| **Preferred Mode of Transport** |  |
| **Other information**  |  |

**ANNEX 2: QUOTATION SUBMISSION FORM**

*Bidders are requested to complete this form, including the Company Profile and Bidder’s Declaration, sign it and return it as part of their quotation along with Annex 3: Technical and Financial Offer. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |
| --- | --- |
| Name of Bidder: | Click or tap here to enter text. |
| RFQ reference: | **RFQ/PAK/December/2022/069** | Date: Click or tap to enter a date. |

**VENDOR INFORMATION SHEET[[1]](#footnote-2) (Attached)**

**BIDDER’S DECLARATION OF CONFORMITY[[2]](#footnote-3)**

| **Yes** | **No** |  |
| --- | --- | --- |
|[ ] [ ]  On behalf of the Supplier, I hereby represent and warrant that neither the Supplier, nor any person having powers of representation, decision-making or control over it or any member of its administrative, management or supervisory body, has been the subject of a final judgement or final administrative decision for one of the following reasons: bankruptcy, insolvency or winding-up procedures; breach of obligations relating to the payment of taxes or social security contributions; grave professional misconduct, including misrepresentation, fraud; corruption; conduct related to a criminal organisation; money laundering or terrorist financing; terrorist offences or offences linked to terrorist activities; child labour and other trafficking in human beings, any discriminatory or exploitative practice, or any practice that is inconsistent with the rights set forth in the Convention on the Rights of the Child or other prohibited practices; irregularity; creating or being a shell company. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier is financially sound and duly licensed. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier has adequate human resources, equipment, competence, expertise and skills necessary to complete the contract fully and satisfactorily, within the stipulated completion period and in accordance with the relevant terms and conditions. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier complies with all applicable laws, ordinances, rules and regulations.  |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier will in all circumstances act in the best interests of IOM. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that no official of IOM or any third party has received from, will be offered by, or will receive from the Supplier any direct or indirect benefit arising from the contract. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier has not misrepresented or concealed any material facts during the contracting process. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier will respect the legal status, privileges and immunities of IOM as an intergovernmental organization. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that neither the Supplier nor any persons having powers of representation, decision-making or control over the Supplier or any member of its administrative, management or supervisory body are included in the most recent Consolidated United Nations Security Council Sanctions List (the “UN Sanctions List”) or are the subject of any sanctions or other temporary suspension. The Supplier will immediately disclose to IOM if it or they become subject to any sanction or temporary suspension.  |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier does not employ, provide resources to, support, contract or otherwise deal with any person, entity or other group associated with terrorism as per the UN Sanctions List and any other applicable anti-terrorism legislation. |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that, the Supplier will apply the highest ethical standards, the principles of efficiency and economy, equal opportunity, open competition and transparency, and will avoid any conflict of interest.  |
|[ ] [ ]  On behalf of the Supplier, I further represent and warrant that the Supplier undertakes to comply with the Code of Conduct, available at <https://www.ungm.org/Public/CodeOfConduct>. |
|[ ] [ ]  It is the responsibility of the Supplier to inform IOM immediately of any change to the information provided in this Declaration. |
|[ ] [ ]  On behalf of the Supplier, I certify that I am duly authorized to sign this Declaration and on behalf of the Supplier I agree to abide by the terms of this Declaration for the duration of any contract entered into between the Supplier and IOM.  |
|[ ] [ ]  IOM reserves the right to terminate any contract between IOM and the Supplier, with immediate effect and without liability, in the event of any misrepresentation made by the Supplier in this Declaration.  |

Signature:

Name: Click or tap here to enter text.

Title: Click or tap here to enter text.

Date: Click or tap to enter a date.

## **ANNEX 3: TECHNICAL AND FINANCIAL OFFER - GOODS**

*Bidders are requested to complete this form, sign it and return it as part of their bid along with Annex 2: Quotation Submission Form. The Bidder shall fill in this form in accordance with the instructions indicated. No alterations to its format shall be permitted and no substitutions shall be accepted.*

|  |  |  |
| --- | --- | --- |
| Name of Bidder: | Click or tap here to enter text. | PR  |
| RFQ reference: | **RFQ/PAK/December/2022/069** | Date: Click or tap to enter a date. |

|  |
| --- |
| **Currency of the Quotation: PKR****INCOTERMS:** Click or tap here to enter text. |
| **Item No** | **Description** | **UOM** | **Qty** | **Unit price** | **Total price**  |
| 1. 1
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Jahangeer Abad, Kuchlak. |  | Civil Works /Rehabilitation  |  |  |
| 1. 2
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Sanzar Khel, Kuchlak. |  | Civil Works /Rehabilitation |  |  |
| 1. 3
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Kechi Baig, Quetta. |  | Civil Works /Rehabilitation |  |  |
| 1. 4
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Kot Waal, Quetta. |  | Civil Works /Rehabilitation |  |  |
| 1. 5
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Kharotabad, Quetta. |  | Civil Works /Rehabilitation |  |  |
| 1. 6
 | Supply and installation of complete pumping machinery and Refurbishment Works of Pump House at Water Supply Scheme (WSS) of Killi Sheikh Maanda Ziarat, Quetta. |  | Civil Works /Rehabilitation |  |  |
| **Total Price** |  |
| **Transportation Price** | **N/A** |
| **Insurance Price** | **N/A** |
| **Installation Price** | **N/A** |
| **Training Price** | **N/A** |
| **Other Charges (specify)** |  |
| **Total Final and All-inclusive Price** |  |
| **Bid Validity Period (in days)** |  |
| **Delivery Time (in days)** |  |

**Notes: Please provide detailed cost in separately attached BoQs.**

**Compliance with Requirements**

|  |  |
| --- | --- |
|  | **You Responses** |
|  | **Yes, we will comply** | **No, we cannot comply** | **If you cannot comply, pls. indicate counter proposal** |
| Minimum Technical Specifications |[ ] [ ]  Click or tap here to enter text. |
| Delivery Term (INCOTERMS) |[ ] [ ]  Click or tap here to enter text. |
| Delivery Lead Time |[ ] [ ]  Click or tap here to enter text. |
| Warranty and After-Sales Requirements |[ ] [ ]  Click or tap here to enter text. |
| Validity of Quotation |[ ] [ ]  Click or tap here to enter text. |
| Payment terms |[ ] [ ]  Click or tap here to enter text. |
| Other requirements *[pls. specify]* |[ ] [ ]  Click or tap here to enter text. |

**Other Information:**

|  |  |
| --- | --- |
| Estimated weight/volume/dimension of the Consignment:  |  Click or tap here to enter text. |
| Country/ies of Origin: (*if export licence required this must be submitted if awarded the contract*) | Click or tap here to enter text. |

|  |
| --- |
| I, the undersigned, certify that I am duly authorized to sign this quotation and bind the company below in event that the quotation is accepted. |
| *Exact name and address of the company*Company NameClick or tap here to enter text.Address: Click or tap here to enter text. Click or tap here to enter text.Phone No.: Click or tap here to enter text.Email Address: Click or tap here to enter text. | Authorized Signature: Date: Click or tap here to enter text.Name: Click or tap here to enter text.Functional Title of Authorised Signatory: Click or tap here to enter text.Email Address: Click or tap here to enter text. |

1. [Vendor Information Sheet.xlsx](https://iomint.sharepoint.com/%3Ax%3A/t/ManilaSupplyChainUnit/EcdiXZEFetxEl29DHqMnNLgBnUvABCGiNC-UMMSpf4ddXQ?e=IBVJfN) [↑](#footnote-ref-2)
2. This form is mandatory to fill in and sign by every vendor who submits quotation [↑](#footnote-ref-3)